|  |
| --- |
| Deep-learning approach to the iron concentration evaluation in silicon solar cell |
|  |
| Olikh Oleg |
| Taras Shevchenko National University of Kyiv, Kyiv, Ukraine, olegolikh@knu.ua,  ORCID: 0000-0003-0633-5429 |
| Lozitsky Oleg |
| Taras Shevchenko National University of Kyiv, Kyiv, Ukraine, olozitsky@gmail.com,  ORCID: 0000-0002-6872-6655 |
| Zavhorodnii Oleksii |
| Taras Shevchenko National University of Kyiv, Kyiv, Ukraine, nevermor464@gmail.com,  ORCID: 0000-0001-8080-766 |

|  |  |
| --- | --- |
| *Cite this paper as:* | *Olikh, O, Lozitsky, O, Zavhorodnii,O.Deep-learning approach to the iron concentration evaluation in silicon solar cell. 9th Eur. Conf. Ren. Energy Sys.21-23April 2021, Istanbul, Turkey* |

|  |  |
| --- | --- |
| **Abstract:** | Impurities are crucial for solar cell (SC) performance. The aim of our work is to show the possibility of fast and easy evaluation of iron concentration in silicon SC by using current-voltage characteristics (IVC). For this purpose, SCAPS was used to simulate the IVCs for *n*+-*p*-*p*+-Si structures with various both base thickness (150-240 μm) and boron doping level (1015-1017 cm-3) in range 290-340 K. The recombination was considered to be associated with iron atoms with concentration 1010-1013 cm-3 and two cases (the coexistence of interstitial atoms Fei and pairs FeiBs as well as the presence of Fei only) were under investigation. The IVC ideality factors were calculated in these cases (*n*Fe-FeB and *n*Fe respectively).*n* values and SC parameters for more than 10,000 structures were used for neural network learning.API Keras was used to construct the network with up to 4 hidden dense layers (up to 300 neuron, relu activation) and iron concentration as output. It has been shownthat mean squared relative error for test data prediction was up to 0.28 in case of network, which trained by *n*Fe-FeB value and up to 0.06 in case of both *n*Fe-FeB and *n*Fe using. |
| ***Keywords****:* | *silicon solar cell, iron concentration,* *neural network, ideality factor* |

© 2021 Published by ECRES

**ACKNOWLEDGMENT**

The work was supported by National Research Foundationof Ukraine by the state budget finance (project 2020.02/0036”Development of physical base of both acoustically controlledmodification and machine learning–oriented characterizationfor silicon solar cells”)